Next: XBM Images, Previous: Image Formats, Up: Images [Contents][Index]

#### 37.17.2 Image Descriptors

An image descriptor is a list which specifies the underlying data for an image, and how to display it. It is typically used as the value of a `display` overlay or text property (see Other Display Specs); but See Showing Images, for convenient helper functions to insert images into buffers.

Each image descriptor has the form `(image . props)`, where props is a property list of alternating keyword symbols and values, including at least the pair `:type type` that specifies the image type.

The following is a list of properties that are meaningful for all image types (there are also properties which are meaningful only for certain image types, as documented in the following subsections):

`:type type`

  The image type. See Image Formats. Every image descriptor must include this property.

`:file file`

  This says to load the image from file file. If file is not an absolute file name, it is expanded in `data-directory`.

`:data data`

  This specifies the raw image data. Each image descriptor must have either `:data` or `:file`, but not both.

  For most image types, the value of a `:data` property should be a string containing the image data. Some image types do not support `:data`; for some others, `:data` alone is not enough, so you need to use other image properties along with `:data`. See the following subsections for details.

`:margin margin`

  This specifies how many pixels to add as an extra margin around the image. The value, margin, must be a non-negative number, or a pair `(x . y)` of such numbers. If it is a pair, x specifies how many pixels to add horizontally, and y specifies how many pixels to add vertically. If `:margin` is not specified, the default is zero.

`:ascent ascent`

  This specifies the amount of the image’s height to use for its ascent—that is, the part above the baseline. The value, ascent, must be a number in the range 0 to 100, or the symbol `center`.

  If ascent is a number, that percentage of the image’s height is used for its ascent.

  If ascent is `center`, the image is vertically centered around a centerline which would be the vertical centerline of text drawn at the position of the image, in the manner specified by the text properties and overlays that apply to the image.

  If this property is omitted, it defaults to 50.

`:relief relief`

  This adds a shadow rectangle around the image. The value, relief, specifies the width of the shadow lines, in pixels. If relief is negative, shadows are drawn so that the image appears as a pressed button; otherwise, it appears as an unpressed button.

`:conversion algorithm`

  This specifies a conversion algorithm that should be applied to the image before it is displayed; the value, algorithm, specifies which algorithm.

  `laplace`
  `emboss`

    Specifies the Laplace edge detection algorithm, which blurs out small differences in color while highlighting larger differences. People sometimes consider this useful for displaying the image for a disabled button.

  `(edge-detection :matrix matrix :color-adjust adjust)`

    Specifies a general edge-detection algorithm. matrix must be either a nine-element list or a nine-element vector of numbers. A pixel at position x/y in the transformed image is computed from original pixels around that position. matrix specifies, for each pixel in the neighborhood of x/y, a factor with which that pixel will influence the transformed pixel; element 0 specifies the factor for the pixel at x-1/y-1, element 1 the factor for the pixel at x/y-1 etc., as shown below:

          (x-1/y-1  x/y-1  x+1/y-1
           x-1/y    x/y    x+1/y
           x-1/y+1  x/y+1  x+1/y+1)

    The resulting pixel is computed from the color intensity of the color resulting from summing up the RGB values of surrounding pixels, multiplied by the specified factors, and dividing that sum by the sum of the factors’ absolute values.

    Laplace edge-detection currently uses a matrix of

          (1  0  0
           0  0  0
           0  0 -1)

    Emboss edge-detection uses a matrix of

          ( 2 -1  0
           -1  0  1
            0  1 -2)

  `disabled`

    Specifies transforming the image so that it looks disabled.

`:mask mask`

  If mask is `heuristic` or `(heuristic bg)`, build a clipping mask for the image, so that the background of a frame is visible behind the image. If bg is not specified, or if bg is `t`, determine the background color of the image by looking at the four corners of the image, assuming the most frequently occurring color from the corners is the background color of the image. Otherwise, bg must be a list `(red green blue)` specifying the color to assume for the background of the image.

  If mask is `nil`, remove a mask from the image, if it has one. Images in some formats include a mask which can be removed by specifying `:mask nil`.

`:pointer shape`

  This specifies the pointer shape when the mouse pointer is over this image. See Pointer Shape, for available pointer shapes.

`:map map`

  This associates an image map of hot spots with this image.

  An image map is an alist where each element has the format `(area id plist)`. An area is specified as either a rectangle, a circle, or a polygon.

  A rectangle is a cons `(rect . ((x0 . y0) . (x1 . y1)))` which specifies the pixel coordinates of the upper left and bottom right corners of the rectangle area.

  A circle is a cons `(circle . ((x0 . y0) . r))` which specifies the center and the radius of the circle; r may be a float or integer.

  A polygon is a cons `(poly . [x0 y0 x1 y1 ...])` where each pair in the vector describes one corner in the polygon.

  When the mouse pointer lies on a hot-spot area of an image, the plist of that hot-spot is consulted; if it contains a `help-echo` property, that defines a tool-tip for the hot-spot, and if it contains a `pointer` property, that defines the shape of the mouse cursor when it is on the hot-spot. See Pointer Shape, for available pointer shapes.

  When you click the mouse when the mouse pointer is over a hot-spot, an event is composed by combining the id of the hot-spot with the mouse event; for instance, `[area4 mouse-1]` if the hot-spot’s id is `area4`.

Function: image-mask-p spec &optional frame

  This function returns `t` if image spec has a mask bitmap. frame is the frame on which the image will be displayed. frame `nil` or omitted means to use the selected frame (see Input Focus).

Next: XBM Images, Previous: Image Formats, Up: Images [Contents][Index]